
# SR11电脑刷机教程

**How to burn the firmware for SR11 in Windows computer?**



1. 首先打开电脑的设备管理器

1.Go to device manger page in the Windows computer




2、将电脑USB数据线插入SR11的背板第2个USB口，如上图所示

2. Connect the SR11 to the computer via the second USB port in the back panel. (As shown in the picture above.)


3、按住SR11前面的旋钮，将USB电源线插入SR11的POWER USB口

3. Hold the volume button of the SR11 and connect the USB power supply to the ‘POWER USB’ port of SR11.




此时电脑中将会出现上图所示设备，就可以松开按住SR11旋钮的手了（USB仍保持与电脑连接状态）

When ‘ingenice USB Boot Device’ is shown in the computer, we could stop holding the volume button. (USB connection is kept still)



1. 将飞傲提供的SR11\_burning\_tool.rar压缩包解压，然后拷贝到C盘根目录下，如上图所示

4. Copy ‘SR11\_burning\_tool’ folder to the root directory of the C disk(as shown above)




1. 返回设备管理器界面，找到SR11设备，选中后鼠标右键弹出菜单，选择“更新驱动程序”

5. In device manager page, right click ‘‘ingenice USB Boot Device’’, then select’update driver software’ option




1. 选择“浏览我的电脑以查找驱动程序”

6. Choose’browse my computer for driver software ’




1. 如上图所示，选择刷机工具所在文件夹，选择至driver文件夹，然后确定

7. Click browse and select the the ‘driver’ folder in the burning tool folder, then click ‘confirm’




1. 点击下一步

8. Click next



1. 出现上图提示，说明刷机驱动安装完成

9. The burning driver is installed successfully when the picture above shown.




1. 此时SR11在设备管理器中会变成图中显示设备

10. The SR11 will show as ‘usb cloner device’ in the device manager page now.


11、将SR11的POWER USB线拔出，断开与SR11的连接（SR11的第2个USB线仍保持与电脑连接）

11. Disconnect the USB connection from the SR11 power USB port (The second USB port keeps connecting to computer still)



12、如上图所示路径，双击打开cloner.exe

12. Double click and run ‘cloner.exe’ from burning tool folder



1. 软件打开后如上图所示，有2个窗口（注，2个窗口任意一个都不要关掉），按图中箭头位置点击“开始”（点击后会变成“停止”字样）

13. Two windows will pop up now. (Do not close any one of them) Click the ‘开始’Start option as shown in picture above



14、此时按住SR11的音量旋钮，同时将POWER USB线插入SR11中，刷机工具会识别设备并自动进入刷机状态。此时可以松开手，不用再按住旋钮，等待刷机完成即可

Hold the volume button of the SR11 again and connect the USB power supply to the ‘POWER USB’ port of SR11.The burning tool will detect the SR11 and enter burning mode. We could stop holding and wait the burning progress finishing.

15、如图所示，刷机完成后SR11会自动开机，此时可以拔掉SR11与电脑的USB线，正常使用SR11。刷机工具也可以正常关掉了。

15. After successfully burning, the SR11 will turn on automatically. Now we could disconnect the connection from the computer and use SR11 normally again.