**如何为JA11升级固件**

**How to upgrade the firmware for the JA11**

**注意：在为JA11升级固件之前，建议拔掉电脑上USB接口的其他解码器，以免升级固件失败！**

**Note: Before upgrading the firmware for JA11, it is recommended to unplug other decoders from the USB interface on the computer to avoid firmware upgrade failure!**

**JA11 V2.1固件升级内容：**

1、修复与某些手机一起使用存在滴答声的问题。

**JA11 V2.1 firmware upgrade content:**

1. Fixed the issue of ticking sound when used with certain mobile phones.

**JA11 V2.1固件升级教程：**

**JA11 V2.1 firmware upgrade tutorial:**

1、请使用Windows 10/11系统电脑，安装V5.68.0驱动：

<https://bbs.fiio.com/note/showNoteContent.do?id=201911191752415983705&tid=16>

1. Please use a Windows 10/11 computer and install the V5.68.0 driver:

<https://forum.fiio.com/note/showNoteContent.do?id=202105191527366657910&tid=17>


2、驱动安装完成后，将JA11插入电脑的USB接口中，JA11插入耳机，之后打开FiiO控制面板，看是否可以识别JA11：




2. After the driver is installed, plug JA11 into the USB port of the computer, plug JA11 into the headset, and then open the FiiO Control Panel to see if JA11 can be recognized:




3、如果JA11成功被FiiO控制面板识别，此时可以打开文件夹“Upgrade Tool”中的烧录工具“JadeAudio JA11 Upgrade Tool”。点击“Scan”，选择“JadeAudio JA11”，之后再点击“File”，选择固件“JadeAudio JA11\_V2.1.bin”，最后点击“UpGrade”，等待固件升级完成：



3. If JA11 is successfully recognized by the FiiO Control Panel, you can open the burning tool "JadeAudio JA11 Upgrade Tool" in the folder "Upgrade Tool". Click "Scan", select "JadeAudio JA11", then click "File", select the firmware "JadeAudio JA11\_V2.1.bin", and finally click "UpGrade" and wait for the firmware upgrade to complete:



4、当出现“UPGRADE FIRMWARE SUCESS”时，即表明固件升级成功。



4. When “UPGRADE FIRMWARE SUCESS” appears, it means the firmware upgrade is successful.

